fix_modify AtC mesh output command — LAMMPS documentation

\(\renewcommand{\AA}{\text{Å}}\)

# fix_modify AtC mesh output command

## Syntax

    fix_modify <AtC fixID> mesh output <file_prefix>

- AtC fixID = ID of fix atc instance

- mesh output = name of the AtC sub-command

- file_prefix = prefix of various generated output files

## Examples

    fix_modify AtC mesh output meshData

## Description

Command to output mesh and associated data: nodesets, facesets, and elementsets. This data is only output once upon initialization since currently the mesh is static. Creates binary (EnSight, “gold” format) output of mesh data.

## Restrictions

None.

## Related AtC commands

- fix_modify AtC command overview

## Default

None.