fix_modify AtC control mask_direction command — LAMMPS documentation

\(\renewcommand{\AA}{\text{Å}}\)

# fix_modify AtC control mask_direction command

## Syntax

    fix_modify <AtC fixID> control mask_direction <direction> <on|off>

- AtC fixID = ID of fix atc instance

- control mask_direction = name of the AtC sub-command

- direction = select direction

- on or off = Toggles state

## Examples

    fix_modify AtC control mask_direction 0 on

## Description

Command to mask out certain dimensions from the atomic regulator

## Restrictions

None.

## Related AtC commands

- fix_modify AtC command overview