fix_modify AtC mesh add_to_nodeset command — LAMMPS documentation

\(\renewcommand{\AA}{\text{Å}}\)

# fix_modify AtC mesh add_to_nodeset command

## Syntax

    fix_modify <AtC fixID> mesh add_to_nodeset <id> <xmin> <xmax> <ymin> <ymax> <zmin> <zmax>

- AtC fixID = ID of fix atc instance

- mesh create_nodeset = name of the AtC sub-command

- id = id to assign to the collection of FE nodes

- <xmin> <xmax> <ymin> <ymax> <zmin> <zmax> = coordinates of the bounding box that contains the desired nodes to be added

## Examples

    fix_modify AtC mesh add_to_nodeset lbc -12.1 -11.9 -12 12 -12 12

## Description

Command to add nodes to an already existing FE nodeset.

## Restrictions

None

## Related AtC commands

- fix_modify AtC command overview

- fix_modify AtC mesh create_nodeset

## Default

Coordinates are assumed to be in lattice units.