fix_modify AtC sample_frequency command — LAMMPS documentation

\(\renewcommand{\AA}{\text{Å}}\)

# fix_modify AtC sample_frequency command

## Syntax

    fix_modify <AtC fixID> sample_frequency <freq>

- AtC fixID = ID of fix atc instance

- sample_frequency = name of the AtC sub-command

- freq = frequency to sample fields in number of steps

## Examples

    fix_modify AtC sample_frequency 10

## Description

Specifies a frequency at which fields are computed for the case where time filters are being applied.

## Restrictions

Must be used with fix atc hardy and is only relevant when time filters are being used.

## Related AtC commands

- fix_modify AtC command overview

## Default

None.