fix_modify AtC consistent_fe_initialization command — LAMMPS documentation

\(\renewcommand{\AA}{\text{Å}}\)

# fix_modify AtC consistent_fe_initialization command

## Syntax

    fix_modify <AtC fixID> consistent_fe_initialization <on|off>

- AtC fixID = ID of fix atc instance

- consistent_fe_initialization = name of the AtC sub-command

- on or off = switch to activate/deactivate the initial setting of the FE intrinsic field to match the projected MD field

## Examples

    fix_modify AtC consistent_fe_initialization on

## Description

Determines whether AtC initializes FE intrinsic fields (e.g., temperature) to match the projected MD values. This is particularly useful for fully overlapping simulations.

## Restrictions

Can be used with: thermal, two_temperature. Cannot be used with time filtering on. Does not include boundary nodes.

## Related AtC commands

- fix_modify AtC command overview

## Default

Default is off