angle_coeff command — LAMMPS documentation

\(\renewcommand{\AA}{\text{Å}}\)

# angle_coeff command

## Syntax

    angle_coeff N args

- N = numeric angle type (see asterisk form below), or type label

- args = coefficients for one or more angle types

## Examples

    angle_coeff 1 300.0 107.0
    angle_coeff * 5.0
    angle_coeff 2*10 5.0

    labelmap angle 1 hydroxyl
    angle_coeff hydroxyl 300.0 107.0

## Description

Specify the angle force field coefficients for one or more angle types. The number and meaning of the coefficients depends on the angle style. Angle coefficients can also be set in the data file read by the read_data command or in a restart file.

\(N\) can be specified in one of two ways. An explicit numeric value can be used, as in the first example above. Or \(N\) can be a type label, which is an alphanumeric string defined by the labelmap command or in a section of a data file read by the read_data command.

For numeric values only, a wild-card asterisk can be used to set the coefficients for multiple angle types. This takes the form “*” or “*n” or “n*” or “m*n”. If \(N\) is the number of angle types, then an asterisk with no numeric values means all types from 1 to \(N\). A leading asterisk means all types from 1 to n (inclusive). A trailing asterisk means all types from n to \(N\) (inclusive). A middle asterisk means all types from m to n (inclusive).

Note that using an angle_coeff command can override a previous setting for the same angle type. For example, these commands set the coeffs for all angle types, then overwrite the coeffs for just angle type 2:

    angle_coeff * 200.0 107.0 1.2
    angle_coeff 2 50.0 107.0

A line in a data file that specifies angle coefficients uses the exact same format as the arguments of the angle_coeff command in an input script, except that wild-card asterisks should not be used since coefficients for all \(N\) types must be listed in the file. For example, under the “Angle Coeffs” section of a data file, the line that corresponds to the first example above would be listed as

    1 300.0 107.0

The angle_style class2 is an exception to this rule, in that an additional argument is used in the input script to allow specification of the cross-term coefficients. See its doc page for details.

The list of all angle styles defined in LAMMPS is given on the angle_style doc page. They are also listed in more compact form on the Commands angle doc page.

On either of those pages, click on the style to display the formula it computes and its coefficients as specified by the associated angle_coeff command.

## Restrictions

This command must come after the simulation box is defined by a read_data, read_restart, or create_box command.

An angle style must be defined before any angle coefficients are set, either in the input script or in a data file.

## Related commands

angle_style

## Default

none