fix_modify AtC read_restart command — LAMMPS documentation

\(\renewcommand{\AA}{\text{Å}}\)

# fix_modify AtC read_restart command

## Syntax

    fix_modify <AtC fixID> read_restart <file_name>

- AtC fixID = ID of fix atc instance

- read_restart = name of the AtC sub-command

- file_name = name of AtC restart file

## Examples

    fix_modify AtC read_restart restart.mydata.AtC

## Description

Reads the current state of the AtC fields from a named text-based restart file.

## Restrictions

The restart file only contains fields and their time derivatives. The reference positions of the atoms and the commands that initialize the fix are not saved e.g. an identical mesh containing the same atoms will have to be recreated.

## Related AtC commands

- fix_modify AtC command overview

- fix_modify AtC write_restart

## Default

None.