pair_style body/rounded/polygon command — LAMMPS documentation

\(\renewcommand{\AA}{\text{Å}}\)

# pair_style body/rounded/polygon command

## Syntax

    pair_style body/rounded/polygon c_n c_t mu delta_ua cutoff

    c_n = normal damping coefficient
    c_t = tangential damping coefficient
    mu = normal friction coefficient during gross sliding
    delta_ua = multiple contact scaling factor
    cutoff = global separation cutoff for interactions (distance units), see below for definition

## Examples

    pair_style body/rounded/polygon 20.0 5.0 0.0 1.0 0.5
    pair_coeff * * 100.0 1.0
    pair_coeff 1 1 100.0 1.0

## Description

Style body/rounded/polygon is for use with 2d models of body particles of style rounded/polygon. It calculates pairwise body/body interactions which can include body particles modeled as 1-vertex circular disks with a specified diameter. See the Howto body page for more details on using body rounded/polygon particles.

This pairwise interaction between rounded polygons is described in Fraige, where a polygon does not have sharp corners, but is rounded at its vertices by circles centered on each vertex with a specified diameter. The edges of the polygon are defined between pairs of adjacent vertices. The circle diameter for each polygon is specified in the data file read by the read data command. This is a 2d discrete element model (DEM) which allows for multiple contact points.

Note that when two particles interact, the effective surface of each polygon particle is displaced outward from each of its vertices and edges by half its circle diameter (as in the diagram below of a gray and yellow square particle). The interaction forces and energies between two particles are defined with respect to the separation of their respective rounded surfaces, not by the separation of the vertices and edges themselves.

This means that the specified cutoff in the pair_style command is the cutoff distance, \(r_c\), for the surface separation, \(\delta_n\) (see figure below). This is the distance at which two particles no longer interact. If \(r_c\) is specified as 0.0, then it is a contact-only interaction. I.e. the two particles must overlap in order to exert a repulsive force on each other. If \(r_c > 0.0\), then the force between two particles will be attractive for surface separations from 0 to \(r_c\), and repulsive once the particles overlap.

Note that unlike for other pair styles, the specified cutoff is not the distance between the centers of two particles at which they stop interacting. This center-to-center distance depends on the shape and size of the two particles and their relative orientation. LAMMPS takes that into account when computing the surface separation distance and applying the \(r_c\) cutoff.

The forces between vertex-vertex, vertex-edge, and edge-edge overlaps are given by:

\[\begin{split}F_n &= \begin{cases} k_n \delta_n - c_n v_n & \delta_n \le 0 \\ -k_{na} \delta_n - c_n v_n & 0 < \delta_n \le r_c \\ 0 & \delta_n > r_c \\ \end{cases} \\ F_t &= \begin{cases} \mu k_n \delta_n - c_t v_t & \delta_n \le 0 \\ 0 & \delta_n > 0 \end{cases}\end{split}\]

Note that \(F_n\) and \(F_t\) are functions of the surface separation \(\delta_n = d - (R_i + R_j)\). In this model, when \((R_i + R_j) < d < (R_i + R_j) + r_c\), that is, \(0 < \delta_n < r_c\), the cohesive region of the two surfaces overlap and the two surfaces are attractive to each other.

In Fraige, the tangential friction force between two particles that are in contact is modeled differently prior to gross sliding (i.e. static friction) and during gross-sliding (kinetic friction). The latter takes place when the tangential deformation exceeds the Coulomb frictional limit. In the current implementation, however, we do not take into account frictional history, i.e. we do not keep track of how many time steps the two particles have been in contact nor calculate the tangential deformation. Instead, we assume that gross sliding takes place as soon as two particles are in contact.

The following coefficients must be defined for each pair of atom types via the pair_coeff command as in the examples above, or in the data file read by the read_data command:

- \(k_n\) (energy/distance^2 units)

- \(k_{na}\) (energy/distance^2 units)

Effectively, \(k_n\) and \(k_{na}\) are the slopes of the red lines in the plot above for force versus surface separation, for \(\delta_n < 0\) and \(0 < \delta_n < r_c\) respectively.

## Mixing, shift, table, tail correction, restart, rRESPA info

This pair style does not support the pair_modify mix, shift, table, and tail options.

This pair style does not write its information to binary restart files. Thus, you need to re-specify the pair_style and pair_coeff commands in an input script that reads a restart file.

This pair style can only be used via the pair keyword of the run_style respa command. It does not support the inner, middle, outer keywords.

## Restrictions

These pair styles are part of the BODY package. They are only enabled if LAMMPS was built with that package. See the Build package page for more info.

This pair style requires the newton setting to be “on” for pair interactions.

## Related commands

pair_coeff

## Default

none

(Fraige) F. Y. Fraige, P. A. Langston, A. J. Matchett, J. Dodds, Particuology, 6, 455 (2008).